IFC building model
Schema: "IFC4"
Description: "ViewDefinition [DesignTransferView_V1.0]"
Time stamp: "2022-02-28T09:29:20"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "22.0.2.392 - Exporter 22.0.2.392 - Alternativ-UI 22.0.2.392"
Application: "Autodesk Revit 2022 (DEU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (DEU)"

People and organizations
  Person "Matthias" "Müller" of Organization "Karlsruher Institut für Technologie"
  Owner history of Person "Matthias" "Müller" of Organization "Karlsruher Institut für Technologie" | application "Autodesk Revit 2022 (DEU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (DEU)" | change NOCHANGE | created 1645808303 (2022-02-25T16:58:23Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  CURRENCY: €
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 48° 8′ 15.359802″ | longitude 11° 34′ 47.783432″ | elevation above sea level 0.
    contains 1 element
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Elastomerlager Lag 9 6MN" | object type "Elastomerlager:Elastomerlager Lag 9 6MN" | names: "Elastomerlager:Elastomerlager Lag 9 6MN:2476260" | material: "<Unnamed>" | property sets: Pset_IntegPlan

Types
  IFCBUILDINGELEMENTPROXYTYPE "Elastomerlager Lag 9 6MN" | 1 occurrence | material: "<Unnamed>"

Property sets
  Pset_IntegPlan | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AP_Erneuerung = "0" (IFCIDENTIFIER)
    AP_Nutzung = "0" (IFCIDENTIFIER)
    AP_herstellung = "1,95268315152504" (IFCIDENTIFIER)
    EP_Erneuerung = "0" (IFCIDENTIFIER)
    EP_Nutzung = "0" (IFCIDENTIFIER)
    EP_herstellung = "0,276782125748837" (IFCIDENTIFIER)
    GWP_Erneuerung = "0" (IFCIDENTIFIER)
    GWP_Nutzung = "0" (IFCIDENTIFIER)
    GWP_herstellung = "925,692957464791" (IFCIDENTIFIER)
    IP_Beschreibung = "Verformungslager aus Kautschuk, nach Richtzeichnung Lag 9, allseits beweglich (verformbar), stahlbewehrt, inkl. Lagersockel fuer 6MN (Fy)" (IFCIDENTIFIER)
    IP_Element = "Elastomerlager Lag 9, fuer 6MN (Fy) Lagerreaktion" (IFCIDENTIFIER)
    IP_GUID = "8D5B39-C326-7698-ACF6-C20D5FC3B204" (IFCIDENTIFIER)
    IP_Preis_Erneuerung = "0" (IFCIDENTIFIER)
    IP_Preis_Herstellung = "3813,48" (IFCIDENTIFIER)
    IP_Preis_Nutzung = "0" (IFCIDENTIFIER)
    IP_Referenzeinheit = "Stck" (IFCIDENTIFIER)
    IP_Referenzjahr = "0" (IFCIDENTIFIER)
    IP_Zeit_Erneuerung = "0" (IFCIDENTIFIER)
    IP_Zeit_Nutzung = "0" (IFCIDENTIFIER)
    IP_Zeit_herstellung = "1,3" (IFCIDENTIFIER)
    Nutzungsdauer = "35" (IFCIDENTIFIER)
    ODP_Erneuerung = "0" (IFCIDENTIFIER)
    ODP_herstellung = "7,08222128529631E-10" (IFCIDENTIFIER)
    PE_Erneuerung = "0" (IFCIDENTIFIER)
    PE_Nutzung = "25756,96" (IFCIDENTIFIER)
    PE_herstellung = "14787,0852710614" (IFCIDENTIFIER)
    POCP_Erneuerung = "0" (IFCIDENTIFIER)
    POCP_Nutzung = "0" (IFCIDENTIFIER)
    POCP_herstellung = "0,265265819369986" (IFCIDENTIFIER)
    Versiegelungsfaktor = "1" (IFCIDENTIFIER)